{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Hárok1","Hárok2","Hárok3"],"not_rendered":{"charts":0,"images":37,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Hárok1","index":0,"n_rows":266,"n_cols":9,"rows_kept":266,"cut":false,"hidden":false,"merged":[[257,1,257,7],[258,1,258,7],[252,1,252,7],[242,7,242,8],[242,3,242,6],[243,7,250,8],[253,1,253,7],[254,1,254,7],[255,1,255,7],[256,1,256,7],[219,7,225,8],[235,7,241,8],[226,3,226,6],[226,7,226,8],[227,7,233,8],[234,3,234,6],[234,7,234,8],[211,3,211,6],[211,7,211,8],[212,7,217,8],[218,3,218,6],[218,7,218,8],[191,7,196,8],[202,3,202,6],[202,7,202,8],[203,7,210,8],[177,7,182,8],[184,7,189,8],[190,3,190,6],[190,7,190,8],[183,3,183,6],[183,7,183,8],[162,7,162,8],[163,7,168,8],[169,3,169,6],[169,7,169,8],[148,3,148,6],[148,7,148,8],[170,7,175,8],[176,3,176,6],[176,7,176,8],[149,7,154,8],[155,3,155,6],[155,7,155,8],[156,7,161,8],[162,3,162,6],[135,7,140,8],[141,3,141,6],[141,7,141,8],[142,7,147,8],[127,3,127,6],[127,7,127,8],[128,7,133,8],[134,3,134,6],[134,7,134,8],[112,7,118,8],[119,3,119,6],[119,7,119,8],[120,7,126,8],[103,3,103,6],[103,7,103,8],[104,7,110,8],[111,3,111,6],[111,7,111,8],[90,7,95,8],[96,3,96,6],[96,7,96,8],[97,7,102,8],[58,7,58,8],[35,7,41,8],[83,7,88,8],[89,3,89,6],[89,7,89,8],[43,7,49,8],[13,7,13,8],[20,7,20,8],[27,7,27,8],[75,3,75,6],[75,7,75,8],[50,3,50,6],[58,3,58,6],[67,3,67,6],[67,7,67,8],[68,7,74,8],[59,7,65,8],[51,7,57,8],[50,7,50,8],[0,0,1,8],[5,0,5,2],[5,6,5,8],[27,3,27,6],[6,3,6,6],[6,7,6,8],[13,3,13,6],[20,3,20,6],[7,7,12,8],[82,3,82,6],[82,7,82,8],[21,7,26,8],[14,7,19,8],[76,7,81,8],[34,3,34,6],[42,3,42,6],[28,7,33,8],[34,7,34,8],[42,7,42,8],[419,0,419,6],[420,0,420,6],[421,0,421,6],[422,0,422,6],[423,0,423,6],[424,0,424,6],[425,0,425,6],[259,0,259,6],[260,0,260,6],[261,0,261,6],[262,0,262,6],[263,0,263,6],[264,0,264,6],[265,0,265,6]],"flags":["formulas_cached_only"]}
["Cenník krbových vložiek BLANZEK"]
[]
[{"$nulls":6},"VEĽKOOBCHOD"]
[]
[]
["Cenník platný od 1.03.2009",{"$nulls":5},"Uvedené ceny sú bez DPH"]
[null,null,null,"Blanzek 600 - rovné sklo ",null,null,null,"CENA"]
[null,null,null,"   Výkon 8kw",null,null,null,352.75]
[null,null,null,"   Dymovod-150mm"]
[null,null,null,"   Rozmer čela 590x460mm,hlbka 398mm"]
[null,null,null,"   Hmotnosť : 90kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[null,null,null,"Blanzek 700 - rovné sklo ",null,null,null,"CENA"]
[null,null,null,"   Výkon 10-12kw",null,null,null,454.75]
[null,null,null,"   Dymovod - 200mm"]
[null,null,null,"   Rozmer čela 700x510mm,hlbka 433mm"]
[null,null,null,"   Hmotnosť : 116kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[null,null,null,"Blanzek 700P - panoráma, ohýbané sklo ",null,null,null,"CENA"]
[null,null,null,"   Výkon 10-12kw",null,null,null,665.55]
[null,null,null,"   Dymovod - 200mm"]
[null,null,null,"   Rozmer čela 690x510mm,hlbka 422mm"]
[null,null,null,"   Hmotnosť : 125kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[null,null,null,"Blanzek 700 R - oblúkové sklo ",null,null,null,"CENA"]
[null,null,null,"   Výkon 10-12kw",null,null,null,651.1]
[null,null,null,"   Dymovod - 200mm"]
[null,null,null,"   Rozmer čela 690x510mm,hlbka 425mm"]
[null,null,null,"   Hmotnosť : 125kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[null,null,null,"Blanzek V 700 - otváranie hore a do boku",null,null,null,"CENA"]
[{"$nulls":7},656.2]
[null,null,null,"   Výkon 10-12kw"]
[null,null,null,"   Dymovod 200mm"]
[null,null,null,"   Rozmer čela 736x5547mm, hlbka 479mm"]
[null,null,null,"   Hmotnosť : 182kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[null,null,null,"Blanzek V 700P - otváranie hore a do boku",null,null,null,"CENA"]
[{"$nulls":7},991.95]
[null,null,null,"   Výkon 10-12kw"]
[null,null,null,"   Dymovod 200mm"]
[null,null,null,"   Rozmer čela 784x510mm, hlbka 442mm"]
[null,null,null,"   Hmotnosť : 182kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[null,null,null,"Blanzek V 700R - otváranie hore a do boku",null,null,null,"CENA"]
[{"$nulls":7},991.95]
[null,null,null,"   Výkon 10-12kw"]
[null,null,null,"   Dymovod 200mm"]
[null,null,null,"   Rozmer čela 785x510mm, hlbka 425mm"]
[null,null,null,"   Hmotnosť : 182kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[null,null,null,"Blanzek V 71 - otváranie hore a do boku ",null,null,null,"CENA"]
[{"$nulls":7},866.15]
[null,null,null,"   Výkon 12-15kw"]
[null,null,null,"   Dymovod 200mm"]
[null,null,null,"   Rozmer čela 749x550mm, hlbka 493mm"]
[null,null,null,"   Hmotnosť : 160kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[]
[null,null,null,"Blanzek V 71 CP/CL - hore a do boku ",null,null,null,"CENA"]
[{"$nulls":7},990.25]
[null,null,null,"   Výkon 12-15kw"]
[null,null,null,"   Dymovod 200mm"]
[null,null,null,"   Rozmer čela 755x570mm, hlbka 425 mm"]
[null,null,null,"   Hmotnosť : 155kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[null,null,null,"Blanzek 71 C - zasklené dva boky",null,null,null,"CENA"]
[null,null,null,"   Výkon 12-15kw",null,null,null,944.35]
[null,null,null,"   Dymovod 200mm"]
[null,null,null,"   Rozmer čela 740x530mm, hlbka 425mm"]
[null,null,null,"   Hmotnosť : 140kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[null,null,null,"Blanzek 71 D - priehľadný",null,null,null,"CENA"]
[null,null,null,"   Výkon 12-15kw",null,null,null,960.5]
[null,null,null,"   Dymovod 200mm"]
[null,null,null,"   Rozmer čela 720x530mm, hlbka 460mm"]
[null,null,null,"   Hmotnosť : 110kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[null,null,null,"Blanzek 720 - rovné sklo NOVINKA",null,null,null,"CENA"]
[null,null,null,"   Výkon 8-14kw",null,null,null,528.7]
[null,null,null,"   Dymovod 200mm"]
[null,null,null,"   Rozmer čela 720x520mm, hlbka 425mm"]
[null,null,null,"   Hmotnosť : 135kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[null,null,null,"Blanzek 720 CP/CL - dvojité sklo NOVINKA",null,null,null,"CENA"]
[null,null,null,"   Výkon 8-14kw",null,null,null,790.5]
[null,null,null,"   Dymovod 200mm"]
[null,null,null,"   Rozmer čela 730x520mm, hlbka 425mm"]
[null,null,null,"   Hmotnosť : 135kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[null,null,null,"Blanzek V 73 - otváranie hore a do boku",null,null,null,"CENA"]
[{"$nulls":7},1163.22]
[null,null,null,"   Výkon 13-16kw"]
[null,null,null,"   Dymovod 200mm"]
[null,null,null,"   Rozmer čela 749x550mm, hlbka 513mm"]
[null,null,null,"   Hmotnosť : 170kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[null,null,null,"Blanzek V 73 P- otváranie hore a do boku",null,null,null,"CENA"]
[{"$nulls":7},1227.4]
[null,null,null,"   Výkon 13-16kw"]
[null,null,null,"   Dymovod 200mm"]
[null,null,null,"   Rozmer čela 815x520mm, hlbka 450mm"]
[null,null,null,"   Hmotnosť : 200kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[null,null,null,"Blanzek V 73 R- otváranie hore a do boku",null,null,null,"CENA"]
[{"$nulls":7},1227.4]
[null,null,null,"   Výkon 13-16kw"]
[null,null,null,"   Dymovod 200mm"]
[null,null,null,"   Rozmer čela 815x520 mm, hlbka 505mm"]
[null,null,null,"   Hmotnosť : 200kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[null,null,null,"BeFDIN 660 - rovné sklo",null,null,null,"CENA"]
[null,null,null,"   Výkon 15kw",null,null,null,1070.15]
[null,null,null,"   Dymovod 180mm"]
[null,null,null,"   Rozmer čela 660x570mm, hľbka 577mm"]
[null,null,null,"   Hmotnosť : 237kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[null,null,null,"BeFDIN 660 P - panoráma",null,null,null,"CENA"]
[null,null,null,"   Výkon 15kw",null,null,null,1191.7]
[null,null,null,"   Dymovod 180mm"]
[null,null,null,"   Rozmer čela 660x570mm, hľbka 614mm"]
[null,null,null,"   Hmotnosť : 236kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[null,null,null,"BeFDIN 660 R - oblúkové sklo",null,null,null,"CENA"]
[null,null,null,"   Výkon 15kw",null,null,null,1226.55]
[null,null,null,"   Dymovod 180mm"]
[null,null,null,"   Rozmer čela 660x570mm, hľbka 628mm"]
[null,null,null,"   Hmotnosť : 227kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[null,null,null,"BeF 520 H - rovné sklo, šamot",null,null,null,"CENA"]
[null,null,null,"   Výkon 6kw",null,null,null,528.7]
[null,null,null,"   Dymovod 150mm"]
[null,null,null,"   Rozmer čela 520x570mm, hľbka 408mm"]
[null,null,null,"   Hmotnosť : 90kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[null,null,null,"BeF 700 - rovné sklo, šamot",null,null,null,"CENA"]
[null,null,null,"   Výkon 8,5kw",null,null,null,659.6]
[null,null,null,"   Dymovod 180mm"]
[null,null,null,"   Rozmer čela 700x500mm, hľbka 433mm"]
[null,null,null,"   Hmotnosť : 135kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[null,null,null,"BeF 700 P - rovné sklo, šamot",null,null,null,"CENA"]
[null,null,null,"   Výkon 8,5kw",null,null,null,818.55]
[null,null,null,"   Dymovod 180mm"]
[null,null,null,"   Rozmer čela 690x510 mm, hľbka 442mm"]
[null,null,null,"   Hmotnosť : 145kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[null,null,null,"BeF 700 R - rovné sklo, šamot",null,null,null,"CENA"]
[null,null,null,"   Výkon 8,5kw",null,null,null,818.55]
[null,null,null,"   Dymovod 180mm"]
[null,null,null,"   Rozmer čela 690x510 mm, hľbka 442mm"]
[null,null,null,"   Hmotnosť : 145kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[null,null,null,"BeF 450 - rovné sklo, šamot",null,null,null,"CENA"]
[null,null,null,"   Výkon 7kw",null,null,null,596.7]
[null,null,null,"   Dymovod 150mm"]
[null,null,null,"   Rozmer čela 450x570 mm, hľbka 442mm"]
[null,null,null,"   Hmotnosť : 135kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[null,null,null,"BeF 450 E - rovné sklo, šamot, rohová",null,null,null,"CENA"]
[null,null,null,"   Výkon 7kw",null,null,null,890.8]
[null,null,null,"   Dymovod 180mm"]
[null,null,null,"   Rozmer čela 490x570 mm, hľbka 450mm"]
[null,null,null,"   Hmotnosť : 115kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[null,null,null,"BeF V 700 Extraline - rovné sklo, výsuv",null,null,null,"CENA"]
[null,null,null,"   Výkon 8,5kw",null,null,null,1067.6]
[null,null,null,"   Dymovod 180mm"]
[null,null,null,"   Rozmer čela 670x506 mm, hľbka 487mm"]
[null,null,null,"   Hmotnosť : 180kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[]
[]
[]
[]
[]
[null,null,null,"Tover Extraline - rovné sklo, šamot, výsuv",null,null,null,"CENA"]
[{"$nulls":7},1321.75]
[null,null,null,"   Výkon 15kw"]
[null,null,null,"   Dymovod 180mm"]
[null,null,null,"   Rozmer čela 610x890 mm, hľbka 621mm"]
[null,null,null,"   Hmotnosť : 270kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[]
[]
[null,null,null,"Blanzek 700 Aqua s dochl. Smyčkou",null,null,null,"CENA"]
[null,null,null,"   Výkon: 15/9,5 kW",null,null,null,629.85]
[null,null,null,"   Priemer dymovodu: 200 mm"]
[null,null,null,"   Rozmer čela krbu: 700x510 mm hĺbka 537"]
[null,null,null,"   Hmotnosť: 130 kg"]
[null,null,null,"   Účinnosť: 77%"]
[]
[null,null,null,"Blanzek 730 Aqua bez dochl. Smyčky",null,null,null,"CENA"]
[null,null,null,"   Výkon 22 kW",null,null,null,990.25]
[null,null,null,"   Do teplovod.výmennníka 15,5 kW "]
[null,null,null,"   Účinnosť nad 80 percent"]
[null,null,null,"   Dymovod 200 mm"]
[null,null,null,"   Celkový rozmer 1215x732x710/hl./"]
[null,null,null,"   Hmotnosť 195 kg "]
[]
[null,null,null,"Blanzek 730 Aqua s dochl. Smyčkou",null,null,null,"CENA"]
[null,null,null,"   Výkon 22 kW",null,null,null,1067.6]
[null,null,null,"   Do teplovod.výmennníka 15,5 kW "]
[null,null,null,"   Účinnosť nad 80 percent"]
[null,null,null,"   Dymovod 200 mm"]
[null,null,null,"   Celkový rozmer 1215x732x710/hl./"]
[null,null,null,"   Hmotnosť 195 kg "]
[]
[null,null,null,"Blanzek 730 Aqua P s dochl. Smyčkou",null,null,null,"CENA"]
[null,null,null,"   Výkon 22 kW",null,null,null,1304.75]
[null,null,null,"   Do teplovod.výmennníka 15,5 kW "]
[null,null,null,"   Účinnosť nad 80 percent"]
[null,null,null,"   Dymovod 200 mm"]
[null,null,null,"   Rozmer čela krbu 720 x 520mm hĺbka 794"]
[null,null,null,"   Hmotnosť 210 kg "]
[]
[null,null,null,"Bef 730 P/R - NOVINKA",null,null,null,"CENA"]
[null,null,null,"   P-prizmatické sklo   R-oblúkové sklo",null,null,null,817.85]
[null,null,null,"   Výkon 8-14,5kw"]
[null,null,null,"   Dymovod 180mm"]
[null,null,null,"   Rozmer čela 720x508 mm, hľbka 534mm"]
[null,null,null,"   Hmotnosť : 155kg"]
[null,null,null,"   Primárne, sekundárne, terciálne horenie"]
[null,null,null,"   Podstavec nie je súčasťou KV"]
[]
["Príslušenstvo Blanzek",{"$nulls":5},"Veľkoobchod",null,"bez DPH"]
[null,"pozinkované opláštenie dľa zvoleného typu",{"$nulls":6},"92,-€"]
[null,"podstavec výškovo nastaviteľný pre radu B",{"$nulls":6},"43,-€"]
[null,"podstavec pre radu BEF, BEF DIN",{"$nulls":6},"68,-€"]
[]
[]
[]
[]
["TUMA INVEST spol.s r.o."]
["Partizánska ul. 300/32, 95701 Bánovce nad Bebravou"]
["Tel:       0905 394 055, 0918 995 337, 0918 463 930"]
["Fax:      038/7600182 "]
["E-mail:  tumainvest@gmail.com"]
["Web:  www.krby-tuma.sk , www.edilkamin-slovakia.sk"]
["           www.kominy-tuma.sk , www.hoyan.sk"]

{"sheet":"Hárok2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Hárok3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}